REQUIRED GLOBE VALVE WITH THE SPECIFICATION

GLOBE VALVE : SDNR 200NB, 10 K, GM

REQUIRED

FLANGE OD:335MM

PCD: 292MM

HOLE: 18MM DIA X8 NOS